// Copyright (C) 2023 The Qt Company Ltd.
// SPDX-License-Identifier: LicenseRef-Qt-Commercial OR GFDL-1.3-no-invariants-only

/*!
    \example satelliteinfo
    \title Satellite Info
    \examplecategory {Application Examples}
    \examplecategory {Positioning & Location}
    \meta tags {c++, qml, quick}

    \brief The Satellite Info example shows the available satellites
    using Sky View, Table View, or RSSI View and the user's current position.
    It is implemented with \l{Qt Positioning} and \l{Qt Quick}.

    \ingroup qtpositioning-examples

    This example demonstrates the usage of \l {Qt Positioning QML Types}
    {Qt Positioning QML API}:

    \list
        \li \l {PositionSource}
        \li \l {SatelliteSource}
    \endlist

    The example also shows how to use a custom \c {C++} model together with a
    custom proxy model from \c {QML}.

    \section1 UI Overview

    The example shows satellite information in three different tabs.
    The data is taken from the \l {SatelliteSource::satellitesInView} and
    \l {SatelliteSource::satellitesInUse} properties.

    \image ../images/skyview_tableview.webp {Satellite view and table UI}

    The \e {Sky View} tab shows the relative satellite positions using the
    \c {Azimuth} and \c {Elevation} \l {geoSatelliteInfo::attribute}
    {attributes}. Clicking on an individual satellite object opens a popup
    with the \l {geoSatelliteInfo::satelliteIdentifier} {satellite identifier},
    its azimuth and elevation.

    The \e {Table View} tab shows the list of all detected satellites, and
    allows to apply sorting and filtering to the list.

    \image ../images/rssiview_settings.webp {RSSI view with satellite signal bars}

    The \e {RSSI View} tab shows the signal strength of satellites in view using
    the \l {geoSatelliteInfo::}{signalStrength} property. The numbers below the
    bars represent the individual \l {geoSatelliteInfo::satelliteIdentifier}
    {satellite identifiers}.

    The \e {Sky View} and \e {RSSI View} tabs also show the current latitude and
    longitude. They use \l {PositionSource::position} property to extract this
    information.

    The \e {Status} block on top of the tabs shows the current mode or the last
    error.

    The \e {Settings} menu allows to switch the application color mode and show
    the help information.

    The application operates in three different modes:

    \table
        \header
            \li Application mode
            \li Description
        \row
            \li Running
            \li The application continuously queries the system for satellite
                and position updates. When new data is available it will be
                displayed.
        \row
            \li Stopped
            \li The application stops updating the satellite and position
                information.
        \row
            \li Single
            \li The application makes a single satellite and position update
                request.
    \endtable

    The application automatically switches into a simulation mode if the
    platform does not provide satellite or position information. The simulation
    mode uses an \l {Qt Positioning NMEA plugin}{NMEA plugin} with pre-recorded
    NMEA data.

    \note Apple does not provide any APIs to retrieve satellite information, so
    on \c macOS and \c iOS the satellite information will always be taken from
    pre-recorded data. These API limitations do not affect positioning
    information, so current position can be displayed correctly.

    \include examples-run.qdocinc

    \section1 Retrieving Current Position

    The current position is retrieved from the \l PositionSource QML object. The
    \c {onPositionChanged} handler is used to receive position updates. The
    string representations of latitude and longitude are extracted from the
    \l {Position::}{coordinate} property.

    \snippet satelliteinfo/ApplicationScreen.qml 3
    \snippet satelliteinfo/ApplicationScreen.qml 4
    \snippet satelliteinfo/ApplicationScreen.qml 5

    \section1 Retrieving Satellite Information

    Similarly to the position, the current satellite information is retrieved
    from the \l SatelliteSource QML object. The \c {onSatellitesInViewChanged}
    and \c {onSatellitesInUseChanged} handlers are used to get the updated
    satellites in view and satellites in use respectively. In this example, the
    data is then forwarded to the \c {C++} model, which is later used in all
    views.

    \snippet satelliteinfo/ApplicationScreen.qml 0
    \snippet satelliteinfo/ApplicationScreen.qml 1
    \snippet satelliteinfo/ApplicationScreen.qml 2

    \note The example shows both the QML Positioning API, and the integration
    of C++ model to QML. That is the reason why the satellite information is
    first retrieved in \c {QML}, then forwarded to \c {C++}, and then back to
    \c {QML} to be used in the model. In practice, if the application is
    supposed to use complex \c {C++} models, consider directly using the
    \l QGeoSatelliteInfoSource class from \c {C++}.

    \section1 Using Custom C++ Models

    The example makes use of two custom models - \c {SatelliteModel} and
    \c {SortFilterModel}.

    \section2 Satellite Model

    The \c {SatelliteModel} class is derived from \l QAbstractListModel and
    reimplements the \l {QAbstractListModel::}{rowCount()},
    \l {QAbstractListModel::}{data()}, and
    \l {QAbstractListModel::}{roleNames()} methods to represent the
    satellite information. Using \l QAbstractListModel as a base class allows
    to easily use the model with the \c {QML} \l ListView and \l Repeater types.
    A custom \c {size} property is used only in the \e {RSSI View} tab to
    dynamically calculate the width of the tab bars.

    \snippet satelliteinfo/satellitemodel.h 0
    \snippet satelliteinfo/satellitemodel.h 1

    The \c {roleNames()} method is used to map the model's roles to the
    property names which can be used to access the model data from \c {QML}.
    For example, the \c {id} name is used to extract the satellite identifier,
    and the \c {rssi} name is used to get the signal strength.

    \snippet satelliteinfo/satellitemodel.cpp 0

    On the \c {QML} side, we can use these names to get the actual values.
    For example, the implementation of \e {RSSI View} uses the \c {rssi},
    \c {inUse}, and \c {id} role names to draw the bars that represent
    individual satellites:

    \snippet satelliteinfo/RssiView.qml 0

    \section2 Proxy Model

    The \c {SortFilterModel} class is used to provide custom sorting and
    filtering of the satellite objects shown in the \e {Table View} tab.

    The model is derived from \l QSortFilterProxyModel and reimplements the
    \l {QSortFilterProxyModel::}{filterAcceptsRow()} and
    \l {QSortFilterProxyModel::}{lessThan()} methods to provide filtering and
    sorting. The model also exposes several \c {slots} to tune the filtering
    and sorting behavior.

    \snippet satelliteinfo/sortfiltermodel.h 0
    \snippet satelliteinfo/sortfiltermodel.h 1

    These slots can be called from both \c {C++} and \c {QML}. For example, the
    \e {Satellite Identifier} delegate uses the \c {updateSelectedSystems()}
    slot to show or hide the information about satellites belonging to certain
    satellite systems. Likewise, the \e {Satellite Status} delegates use the
    \c {updateShowInView()} and \c {updateShowInUse()} slots to filter the
    satellites with a specific status.

    \snippet satelliteinfo/SatelliteView.qml 0
    \dots
    \snippet satelliteinfo/SatelliteView.qml 1

    \section1 QML Module Registration

    \section2 CMake Build

    For a CMake-based build, we need to add the following to the
    \c {CMakeLists.txt}:

    \quotefromfile satelliteinfo/CMakeLists.txt
    \skipto qt_add_qml_module(satelliteinfo
    \printuntil )

    \section2 qmake Build

    For a qmake build, we need to modify the \c {satelliteinfo.pro} file in the
    following way:

    \quotefromfile satelliteinfo/satelliteinfo.pro
    \skipto CONFIG += qmltypes
    \printuntil QML_IMPORT_MAJOR_VERSION = 1
    \skipto qml_resources.files
    \printuntil RESOURCES += icon_resources
*/
